|  |
| --- |
| **PRODUCT INFORMATION** |
| 600 Series Cast Iron Wheel Caster |
| 600\*\*-\*\*\*\*\*\*R-01 |
|  |
| Wanda Cast Iron Casters also known as Gray Iron Casters are fully metal wheels and are less expensive than Ductile Wheels. Semi Steel wheels are better for light to medium duty applications if used on smooth concrete floors and applications where they do not take any type of overloading, impacts, or abuse.Temperature Range: -45℃ to +300℃, and Hardness: HBW 180 |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Wheel****Dia.****D** | **Tread****Width****W** | **Load****Cap.****(kg)** | **Bearing****Options** | **Swivel****Radius****E** | **Overall****Height****H** | **Plate****Size****XxY** | **Setting****Pitch****X’xY’** | **Hole****Dia.****P** |
| 100 | 50 | 320 | Roller | 31 | 141 | 115x100 | 83x71 | 11 |
| 125 | 50 | 410 | Roller | 41 | 163 | 115x100 | 83x71 | 11 |
| 150 | 50 | 420 | Roller | 44 | 189 | 115x100 | 83x71 | 11 |
| 200 | 50 | 450 | Roller | 44 | 239 | 115x100 | 83x71 | 11 |
| \*All dimention are “mm”. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Wheel****Dia.****D** | **Swivel Caster****Model No.** | **Fixed Caster****Model No.** | **Swivel** **With Total Lock****Model No.** |
| 100 | 600PS-100050R-01 | 600PF-100050R-01 | 600PS-100050R-01-DUC |
| 125 | 600PS-125050R-01 | 600PF-125050R-01 | 600PS-125050R-01-DUC |
| 150 | 600PS-150050R-01 | 600PF-150050R-01 | 600PS-150050R-01-DUC |
| 200 | 600PS-200050R-01 | 600PF-200050R-01 | 600PS-200050R-01-DUC |
| **Wheel****Dia.****D** | **Swivel** **With Side Brake****Model No.** | **Fixed** **With Side Brake****Model No.** |  |
| 100 | 600PS-100050R-01-STC | 600PF-100050R-01-STC |  |
| 125 | 600PS-125050R-01-STC | 600PF-125050R-01-STC |  |
| 150 | 600PS-150050R-01-STC | 600PF-150050R-01-STC |  |
| 200 | 600PS-200050R-01-STC | 600PF-200050R-01-STC |  |

|  |
| --- |
| **Advantages at a glance** |
| Roll performance |[x]  [x]  | [x]  | [x]  | [x]  |  |
| Movement noise | [x]  | [x]  | [ ]  | [ ]  | [ ]  |  |
| Attrition | [x]  | [x]  | [x]  | [x]  | [x]  |  |
| Corrosion resistance | [x]  | [x]  | [x]  | [x]  | [ ]  |  |

|  |  |
| --- | --- |
|

|  |
| --- |
| LOGO**Better Quality, Better Mobility.**  |

 |

|  |
| --- |
| 4 inch heavy duty fixed casters5 inch heavy duty swivel casters with side brake5 inch heavy duty swivel casters with total lock4 inch heavy duty swivel casters |
| Picture may differ from original product |

|  |
| --- |
| **Dimensions** |

|  |
| --- |
| QQ截图20200924143201 |

|  |
| --- |
| **Stucture & Mounting** |

|  |
| --- |
|  |