|  |
| --- |
| **PRODUCT INFORMATION** |
| 600 Series PU on Alu Wheel Caster |
| 600\*\*-\*\*\*\*\*\*B-73 |
|  |
| Wanda Polyurethane on Aluminium Caster with our High Quality Poly on Aluminum Wheels are used in many applications where the casters and wheels are exposed to water or chemicals. Aluminum is resistant to rust and provides a very strong core for the liquid cast polyurethane tread. Polyurethane on Aluminum wheels are used in Food Processing Equipment, Food Service, Hospitals, Research Laboratories, Pharmaceutical Laboratories, Bakeries, Schools, Institutional, and industrial applications and environments. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Wheel**  **Dia.**  **D** | **Tread**  **Width**  **W** | **Load**  **Cap.**  **(kg)** | **Bearing**  **Options** | **Swivel**  **Radius**  **E** | **Overall**  **Height**  **H** | **Plate**  **Size**  **XxY** | **Setting**  **Pitch**  **X’xY’** | **Hole**  **Dia.**  **P** |
| 100 | 50 | 320 | Ball | 31 | 141 | 115x100 | 83x71 | 11 |
| 125 | 50 | 410 | Ball | 41 | 163 | 115x100 | 83x71 | 11 |
| 150 | 50 | 420 | Ball | 44 | 189 | 115x100 | 83x71 | 11 |
| 200 | 50 | 450 | Ball | 44 | 239 | 115x100 | 83x71 | 11 |
| \*All dimention are “mm”. | | | | | |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Wheel**  **Dia.**  **D** | **Swivel Caster**  **Model No.** | **Fixed Caster**  **Model No.** | **Swivel**  **With Total Lock**  **Model No.** |
| 100 | 600PS-100050B-73 | 600PF-100050B-73 | 600PS-100050B-73-DUC |
| 125 | 600PS-125050B-73 | 600PF-125050B-73 | 600PS-125050B-73-DUC |
| 150 | 600PS-150050B-73 | 600PF-150050B-73 | 600PS-150050B-73-DUC |
| 200 | 600PS-200050B-73 | 600PF-200050B-73 | 600PS-200050B-73-DUC |
| **Wheel**  **Dia.**  **D** | **Swivel**  **With Side Brake**  **Model No.** | **Fixed**  **With Side Brake**  **Model No.** |  |
| 100 | 600PS-100050B-73-STC | 600PF-100050B-73-STC |  |
| 125 | 600PS-125050B-73-STC | 600PF-125050B-73-STC |  |
| 150 | 600PS-150050B-73-STC | 600PF-150050B-73-STC |  |
| 200 | 600PS-200050B-73-STC | 600PF-200050B-73-STC |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Advantages at a glance** | | | | | | |
| Roll performance |  |  |  |  |  |  |
| Movement noise |  |  |  |  |  |  |
| Attrition |  |  |  |  |  |  |
| Corrosion resistance |  |  |  |  |  |  |

|  |  |
| --- | --- |
| |  | | --- | | LOGO  **Better Quality, Better Mobility.** | |

|  |
| --- |
| 4020RP1030025600PS-150050R-13-DUC600PS-150050R-13 |
| Picture may differ from original product |

|  |
| --- |
| **Dimensions** |

|  |
| --- |
| QQ截图20200924143201 |

|  |
| --- |
| **Stucture & Mounting** |

|  |
| --- |
|  |