|  |
| --- |
| **PRODUCT INFORMATION** |
| 600 Series Plastic Wheel Caster |
| 600\*\*-\*\*\*\*\*\*R-05 |
|  |
| Wanda Industrial Plastic (Polyolefin) Wheels also known as Polyolefin Caster Wheels are injection molded from a blend of polyolefin/polypropylene polymers forming a one piece design that is solid and will not de-laminate. Polyolefin Wheels are great for wet and corrosive environments while providing a high impact resistant wheel. Polyolefin wheels are more economical compared to a Phenolic Wheel or a Steel Wheel. These wheels are non-marking and light in weight. Black is the standard color on plastic wheels.  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Wheel****Dia.****D** | **Tread****Width****W** | **Load****Cap.****(kg)** | **Bearing****Options** | **Swivel****Radius****E** | **Overall****Height****H** | **Plate****Size****XxY** | **Setting****Pitch****X’xY’** | **Hole****Dia.****P** |
| 100 | 50 | 230 | Roller | 31 | 141 | 115x100 | 83x71 | 11 |
| 125 | 50 | 300 | Roller | 41 | 163 | 115x100 | 83x71 | 11 |
| 150 | 50 | 320 | Roller | 44 | 189 | 115x100 | 83x71 | 11 |
| 200 | 50 | 400 | Roller | 44 | 239 | 115x100 | 83x71 | 11 |
| \*All dimention are “mm”. |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Wheel****Dia.****D** | **Swivel Caster****Model No.** | **Fixed Caster****Model No.** | **Swivel** **With Total Lock****Model No.** |
| 100 | 600PS-100050R-05 | 600PF-100050R-05 | 600PS-100050R-05-DUC |
| 125 | 600PS-125050R-05 | 600PF-125050R-05 | 600PS-125050R-05-DUC |
| 150 | 600PS-150050R-05 | 600PF-150050R-05 | 600PS-150050R-05-DUC |
| 200 | 600PS-200050R-05 | 600PF-200050R-05 | 600PS-200050R-05-DUC |
| **Wheel****Dia.****D** | **Swivel** **With Side Brake****Model No.** | **Fixed** **With Side Brake****Model No.** |  |
| 100 | 600PS-100050R-05-STC | 600PF-100050R-05-STC |  |
| 125 | 600PS-125050R-05-STC | 600PF-125050R-05-STC |  |
| 150 | 600PS-150050R-05-STC | 600PF-150050R-05-STC |  |
| 200 | 600PS-200050R-05-STC | 600PF-200050R-05-STC |  |

|  |
| --- |
| **Advantages at a glance** |
| Roll performance |[x]  [x]  | [x]  | [x]  | [ ]  |  |
| Movement noise | [x]  | [x]  | [x]  | [ ]  | [ ]  |  |
| Attrition | [x]  | [x]  | [x]  | [ ]  | [ ]  |  |
| Corrosion resistance | [x]  | [x]  | [x]  | [x]  | [ ]  |  |

|  |  |
| --- | --- |
|

|  |
| --- |
| LOGO**Better Quality, Better Mobility.**  |

 |

|  |
| --- |
| 600PF-150050R-05600PS-150050R-05-STA600PS-150050R-05-DUA600PS-150050R-05 |
| Picture may differ from original product |

|  |
| --- |
| **Dimensions** |

|  |
| --- |
| QQ截图20200924143201 |

|  |
| --- |
| **Stucture & Mounting** |

|  |
| --- |
|  |