|  |
| --- |
| **PRODUCT INFORMATION** |
| 600 Series Plastic Wheel Caster |
| 600\*\*-\*\*\*\*\*\*R-05 |
|  |
| Wanda Industrial Plastic (Polyolefin) Wheels also known as Polyolefin Caster Wheels are injection molded from a blend of polyolefin/polypropylene polymers forming a one piece design that is solid and will not de-laminate. Polyolefin Wheels are great for wet and corrosive environments while providing a high impact resistant wheel. Polyolefin wheels are more economical compared to a Phenolic Wheel or a Steel Wheel. These wheels are non-marking and light in weight. Black is the standard color on plastic wheels. |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Wheel**  **Dia.**  **D** | **Tread**  **Width**  **W** | **Load**  **Cap.**  **(kg)** | **Bearing**  **Options** | **Swivel**  **Radius**  **E** | **Overall**  **Height**  **H** | **Plate**  **Size**  **XxY** | **Setting**  **Pitch**  **X’xY’** | **Hole**  **Dia.**  **P** |
| 100 | 50 | 230 | Roller | 31 | 141 | 115x100 | 83x71 | 11 |
| 125 | 50 | 300 | Roller | 41 | 163 | 115x100 | 83x71 | 11 |
| 150 | 50 | 320 | Roller | 44 | 189 | 115x100 | 83x71 | 11 |
| 200 | 50 | 400 | Roller | 44 | 239 | 115x100 | 83x71 | 11 |
| \*All dimention are “mm”. | | | | | |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Wheel**  **Dia.**  **D** | **Swivel Caster**  **Model No.** | **Fixed Caster**  **Model No.** | **Swivel**  **With Total Lock**  **Model No.** |
| 100 | 600PS-100050R-05 | 600PF-100050R-05 | 600PS-100050R-05-DUC |
| 125 | 600PS-125050R-05 | 600PF-125050R-05 | 600PS-125050R-05-DUC |
| 150 | 600PS-150050R-05 | 600PF-150050R-05 | 600PS-150050R-05-DUC |
| 200 | 600PS-200050R-05 | 600PF-200050R-05 | 600PS-200050R-05-DUC |
| **Wheel**  **Dia.**  **D** | **Swivel**  **With Side Brake**  **Model No.** | **Fixed**  **With Side Brake**  **Model No.** |  |
| 100 | 600PS-100050R-05-STC | 600PF-100050R-05-STC |  |
| 125 | 600PS-125050R-05-STC | 600PF-125050R-05-STC |  |
| 150 | 600PS-150050R-05-STC | 600PF-150050R-05-STC |  |
| 200 | 600PS-200050R-05-STC | 600PF-200050R-05-STC |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Advantages at a glance** | | | | | | |
| Roll performance |  |  |  |  |  |  |
| Movement noise |  |  |  |  |  |  |
| Attrition |  |  |  |  |  |  |
| Corrosion resistance |  |  |  |  |  |  |

|  |  |
| --- | --- |
| |  | | --- | | LOGO  **Better Quality, Better Mobility.** | |

|  |
| --- |
| 600PF-150050R-05600PS-150050R-05-STA600PS-150050R-05-DUA600PS-150050R-05 |
| Picture may differ from original product |

|  |
| --- |
| **Dimensions** |

|  |
| --- |
| QQ截图20200924143201 |

|  |
| --- |
| **Stucture & Mounting** |

|  |
| --- |
|  |